**SS202SVHMH6S013 –***Heavy-Duty Two Arm (Side-Mount) Spider*

**Product Specifications**

**Specification Summary:**Heavy-Duty Two Arm V-Shaped (Side-Mount) Spider Fitting (SS20): Provide Type 316 finished stainless steel with M12 x 40mm studs (x2) and corresponding cylindrical end caps (x4). Loading capability: lateral load 1.5kN (per leg), tensile load 3.7kN; for compression load, refer to loading capacity of the glass bolt chosen. Need glass bolts to affix spider to glass. Permitted Product: “Model SS202SVHMH6S013” by Stella Glass Hardware; [www.stellaglasshardware.com](http://www.stellaglasshardware.com).  
  
  
  
**Specification Details:**

* Division:
  + 08 88 00: Special Function Glazing
* Materials:
  + Steel: Grade 316 stainless steel
  + Finish: No. 4, 320 grit
* Mount Type: Side-mount
* Mount Structure: Concrete, steel or wood
  + Mounting Substrate Thickness: 6 to 13mm [1/4" to 1/2"]
* Loading Capability: Lateral load 1.5kN (per leg), Tensile load 3.7kN   
  (for compression load, refer to loading capacity of the Stella Glass Bolt chosen)
* LEED Standards:
  + Stainless Steel (primary material) - >45% pre-/95% post- consumer recycled content by weight
* Compliances/Standard: Project specific
* Warranty: 2-year limited warranty\* (can be project specific)